HiMill D1S installer bundle
============================
sender version : 0.7.6
bundle version : 0.7.6
sender defaults: D1S grblHAL machine profile
rotation test  : grblHAL WCS rotation build for GUSender 0.7.6
grblHAL rev    : 5cd9913-dirty
grblHAL binary : grblhal-d1s-5cd9913-dirty.bin
grblHAL size   : 225076 bytes
grblHAL sha256 : 93f69c3f32a35399fa3ca58e11426cd020d7985083d0e2e785f0b346eaff2e6c
ESP3D firmware : firmware_V1.0.2_20260407.bin
ESP3D sha256   : 59be9cc85e852597ef764b3edbf391c08b56c37d342c568c11b2dcfa3b1abcbf
built          : 2026-05-16T20:00:41-05:00
host           : cbolly
